# Namespace EchoHub.Core.Constants | EchoHub Documentation

# Namespace EchoHub.Core.Constants

### Classes

HubConstants

MessageConventions

  Cross-protocol message conventions. Action messages (`/me`) use the IRC CTCP ACTION wire format 0x01 + "ACTION " + text + 0x01 as the stored content, so IRC clients interoperate natively (irssi's /me arrives in exactly this shape) and the TUI renders "* nick text". In end-to-end encrypted rooms the marker encrypts along with the text.

ValidationConstants